CITY OF SCOTT LOUISIANA

PURCHASE OF ONE (1) OR MORE SIXTEEN (16) YARD, TANDEM AXLE DUMP TRUCKS

**City of Scott, Louisiana wants to purchase One (1) or more 2018-2019 Tandem Dump Trucks with sixteen (14) Yard Dump Bodies shall be new for which the published specifications are available. Bid pricing will be placed by a reverse auction and will be submitted electronically on Thursday, August 16,2018, commencing at 11:30 a.m. and ending at 12:30 p.m. Equipment modifications to meet the operational requirements of this specification shall be limited to manufactures published standard and optional equipment. The equipment shall meet all OSHA and EPA requirements in effect as of this date.**

**All items are to be marked in the specification response below with a Yes or No. For any line marked with a no a complete explanation for the alternate must be in written form and accompany this package. By not completing this package in its entirety will disqualify the Suppliers from bidding. The City of Scott reserves the right to reject all bids or any part of the bid and waive any informality. All equipment offered in bid must meet or exceed these specifications in both performance and quality. Any brand-name specifications are used to denote quality or performance standards only. Any truck meeting or exceeding the specifications will be considered.**

All documents including brochures must be submitted by uploading to the EASiBuy platform or sent via courier the City of Scott no later than Monday, August 13, 2018 on or before 5:00 P.M. If sent by courier the document package must be delivered to Shelly M. Gautreau, City Clerk, City of Scott, 125 Lions Club Rd. Scott, Louisiana, 70583.

In the event of any questions regarding the specification’s, contact Keith Theriot, Superintendent by Phone 337-889-5032, extension #5032 or email at: [keith@cityofscott.org](file:///C%3A%5CUsers%5CFrank%5CAppData%5CLocal%5CMicrosoft%5CWindows%5CTemporary%20Internet%20Files%5CContent.Outlook%5CX72J1531%5Ckeith%40cityofscott.org).

# YES NO

1. Truck & Chassis with a 16-Cubic Yard, minimum 14-Foot-Long Dump Body Warren Model U650, color Black, or equivalent that must meet general dimensions for length, width, height and structure thickness and capacity. Tailgate latch to be air actuated. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
2. Dump Body to have cab protector, LED lighting and have a PTO driven hydraulic pump. Hoist is to be a U110-8824, class 110, NTEA type V twin cylinder underbody hoist with 39 plus ton capacity. Body & hoist must be one manufacture to preclude any problems of mating and warranty. Dump Body shall be equipped with two (2) OSHA approved body props. Dump body to be fully installed and functional when delivered. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
3. Aluminum Conventional Cab Freightliner-color White, M2-106 or comparable. 106 in’ roof with Tandem Axles, Rear Dual Wheels. Wheel base 177 inches +five (5) inches. LH primary steering location, adjustable tilt telescoping steering column with 18 in. +1 inch. Power Steering, Cruise Control, Air brakes front & rear, Two (2) valve parking brake system. Tinted windshield, amber lights on cab roof. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
4. Suspension shall be Heavy Duty, Rear Suspension, Minimum of 40,000 lb. Front Suspension shall be 14,700 lb. minimum, GVWR 54,000 lbs. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
5. Heavy Duty Frame Outer Channel shall be heat‐treated steel, Frame to include full frame reinforcement. To include Heavy duty springs front and rear and front Two (2) Tow Hooks, Pintle Hook Military Hitch capacity 45 Ton and two (2) trailer tow hook D-rings. Air connections to end of frame, Seven (7) way RV style trailer connecter receptacle. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
6. Cummins Diesel Engine Minimum 350 HP, governed to 65 MPH, Heavy duty Radiator with two speed fan hub, 18.0 CFM Compressor, Air operated Power takeoff, with switch installed on Truck dash, and bug screen. Exhaust shall be Vertical Exhaust. Equipped with Engine Brake. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
7. Transmission shall be Fully Automatic Allison 3500-RDS Transmission with PTO provision or equal. Push button control electronic shift control, dash mounted. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
8. Cab shall be equipped with Air Ride Cab, HD Vinyl Air Ride high back Drivers Seat air suspension, Passenger Seat, HD Vinyl with air suspension. Hand Throttle, Air Horn and be equipped with armrest, sun visors air conditioned and heat with defrost, AM/FM Radio all standard equipment and tinted glass all around, AM/FM Radio, Blue-tooth equipped with hands free, Radio Hot Post, Console Controls, and Black Vinyl floor covering. Gauges package for Cab to equipped with following gauges Tachometer, Fuel Gauge, and DEF Tank Gauge, Engine coolant, Volt-Ampere Meter, Primary and secondary Air-gauge and Engine Hour Meter. Equipped with minimum five (5) lb. Fire extinguisher, Triangle Warning Kit, two-(2) inch fender extensions. \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
9. Battery & Wiring: Heavy Duty Alternator Battery should be group thirty-one (31) with minimum 2100 cranking amps. Chassis to be wired for multi-function engine connection for body builders to end of frame (EOF). \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
10. Outside cab: Grab Handles, West Coast Mirrors each side, and additional 6 inch round convex mirror on each side below the standard mirror or equivalent down-view mirror. Minimum Fuel Tank Fifty (50) Gallon Minimum Capacity, DEF tank, minimum six (6) gallon. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_
11. Brakes – Air Brakes with Automatic Slack Adjusters, Engine brake. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_
12. Tires & Wheels: shall be equipped with 385/65-R22.5 highway tread, deep lug drive 11R22.5. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_
13. Back-up Alarm, Lights to meet all Federal and State Regulations, and All Standard Equipment. Lights are to be equipped with emergency Strobe type lights. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_
14. Dump Bed 16 Cubic Yard Dump Body with minimum 1/4 Steel floors with cross members located on Twelve (12) inch Centers. Air Tailgate, Asphalt Apron 12 inches long, Backup Alarm, Automatic Electric Roll-A-Way Tarp Cover, and Mud Flaps. Dump Body Color Black. \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_
15. Standard Full Warranty: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Term: \_\_\_\_\_\_ Mile/Hours: \_\_\_\_\_\_. This Warranty is required and will be a factor in determining lowest or best bid. A copy of the Warranty must be included with the Specification Response for review.

1. Option to Bid Additional Extended Full Warranty beyond Standard Warranty: \_\_\_\_\_\_\_ \_\_\_\_\_\_\_
2. Estimated delivery time from date of order. # of days: \_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_

**End of Specifications**